|  |  |  |
| --- | --- | --- |
| Date 23 .03 .2018 |  |  |
| Item 1:Priority of the PES device in SASE3Description The PES has now low priority. JGruenert points out that the PES is necessary for operating SASE3. | Action J.Gruenert will discuss this with CYoungman . Result/decision | Who JG\CY |
| Item 2:XGM SASE3 vacuum issueDescription After restarting of the CPP servers the XGM turbo pumps stopped, valves closed and it required a manual intervention to restore them. | Action The issue can be fixed with a loop update. Today will be discussed when to to do the update. JG would like it as soon as possible. The update has to be coordinated with the PRC not to cause unexpected problems with the beam in SASE1. Result/decision | Who AE\CAS\PRC |